# FAQ - Frequently Asked Questions

#### 2025-08-21

Abstract

A short list of responses and clarifications about Frequently Asked Questions from r5r users.

# 1. Why do some trips from/to the same ID have travel times larger than zero?

click to expand

> This can happen when the input point is distant to any routable road segment. In this case, R5 will snap the point to the closest road segment that can be traversed with the selected transport mode, and it will consider that the person would walk in Euclidean distance from the input point to the snapped location. So R5 is accounting for this walking time “as the crow flies” in the routing.

# 2. Is it possible to run `r5r` with custom modifications to street nework data?

click to expand

> Yes, all routing and accessibility functions in `r5r` have new parameters `new_carspeeds`, `carspeed_scale` and `new_lts` which allow one to use custom car speeds and LTS levels for cycling. These parameters provide convient and efficient ways to build different scenarios of traffic congestion, road closure and interventions in cycling infrastructure. See this vignette. For other changes to the OSM network (e.g. including a new road link), you would need to edit the OpenStreetMap `.pbf` file direclty before using it in `r5r`. To to this, you can edit the `.pbf` file with JOSM (https://wiki.openstreetmap.org/wiki/JOSM). Mind you that the the OpenStreetMap tags can be changed but they cannot be removed from the data.

# 3. Why are the output results of `time_travel_matrix()` and `detailed_itineraries()` different?

click to expand

> The functions `time_travel_matrix()` (and `expanded_time_travel_matrix`) and `detailed_itineraries()` use different routing algorithms, as explained in the documentation of these functions. As such, we advise not to use or combine the output of these functions.

# 4. What does the ERROR “Geographic extent of street layer exceeds limit” mean? and what to do about it?

click to expand

> If you an error message says something like: “Geographic extent of street layer (5315196 km2) exceeds limit of 975000 km2”. This means the your study area is too large. Unfortunately, this is a limit hardcoded upstream in R5 so we cannot change it in r5r. The advised solution here would be to reduce the extent of the `OpenStreetMap.pbf` to a smaller area of interest. One can do this using the Osmosis software. The code below illustrates how to do this by calling Osmosis from within R. You need to donwload the Osmosis program to your computer. The latest releases can be downloaded from here. Next, you can use this step-by-step illustrated in the example below:

    # get the bounding box of your study area
    study_area_polygon <- geobr::read_state(code_state = "ES")
    area_bbox <- sf::st_bbox(study_area_polygon)

    # input: the path to osmosis and the large pbf file in your local computer
    osmosis_path <- "./osmosis_dir/bin/osmosis.bat"
    large_pbf_path <- "./project_dir/large.pbf"

    # path where you want to save the smaller .pbf file
    smaller_pbf <-"./project_dir/smaller.pbf"

    # prepare call to osmosis
    osmosis_cmd <- sprintf("%s --read-pbf %s --bounding-box left=%s bottom=%s right=%s top=%s --write-pbf %s",
                           osmosis_path, large_pbf_path,
                           area_bbox@xmin, area_bbox@ymin, area_bbox@xmax, area_bbox@ymax,
                           smaller_pbf)

    # call to osmosis
    shell(osmosis_cmd, translate = TRUE)

# 5. Is it possible to use custom car speed data with r5r?

click to expand

> By default, R5 considers the max speed limit of each road as set in OpenStreetMap data. Unfortunately, there is currently no easy way to change the car speeds of road segments from within R. Although you could probably do that by editing the osm.pbf file using other programs. See issue #289.

# 6. Why do I get identical results by public transport and walking?

click to expand

> If your travel time / accessibility results are identical for public transport and walking, it is probably because R5 did not detect that the public transport network is available for your requested trips. This is likely to occur in case you set a `departure_datetime` outside the calendar of public transport operations in your GTFS data. Check the `calendar.txt` file in your gtfs.zip feed. Alternatively, this could occur because there is no public transport trip option that would be faster than walking for the given origin-destination pair you queried.